|  |  |
| --- | --- |
| **Potential Hazard if the transfer is NOT performed correctly** | |
|  | * **Contact with Hot Emulsion products** * **Contamination of the Environment due to an Emulsion spill** |
| **Access Rules** | |
| EntreeInterditePersonnesNonAutorisees | * Only competent, authorised personnel are to transfer and receive emulsion from a tanker to a sprayer. * Deliveries must be drawn off the emulsion tanker by the sprayer. * Pressure discharge is forbidden. * Ensure there is a **three** metre exclusion zone to prevent unauthorized access to the transfer activity. * If any unauthorized personnel enter the 3m zone the transfer must stop. * Ensure a safe area to work around the transfer is maintained. * The Sprayer Driver and Emulsion Tanker Driver must be in communication at all times during the transfer. |
| **PPE Rules** | |
| ProtectionObligatoireFigureProtectionObligatoireVueProtectionObligatoireTete ProtectionObligatoireCorps ProtectionObligatoireMains ProtectionObligatoirePieds ProtectionObligatoireOuie | |
| **Environment Rules** | |
|  | * A Safe System of Work must follow Procedure REA Doc No. 002. * Ensure there is sufficient ullage in the receiving sprayer. * Ensure there is suitable spill containment in place at the inlet(s) e.g. Drip bucket? * Extra vigilance must be maintained if the delivery point(s) is within 20 metres of a drain, open water, river, canal, location inclines etc. * A transfer is not permitted if the delivery point(s) **is within 10 metres** of a drain, open water, river, canal etc. * Oil spill kits and drain mats must be available on both vehicles at the transfer point. |

5

